1992 International 2654 6x4 Pumper Tanker. Truck has a DT 466 225hp diesel motor with an Allison automatic transmission. 24,651 miles and 1,713.9 hours on it. Darley 1250gpm pump with a poly 2,250- gallon water tank. Driver's side pump panel has two 2.5" discharges and two 2.5" tank fills. Passenger side pump panel has two 2.5" discharges, one 3" stortz discharge, one 2.5" suction and one 6" steamer. There are two 1 %/" preconnected cross lays. Truck has a removable Deck Gun piped to the top of the truck. LED headlights and back up lights. Has an Electrol Model 18-30 3,000-watt generator runs off the main motor. Truck will come with one 28ft extension ladder, one 16ft roof ladder, and one 10ft attic ladder, three 10ft sections of 6" hard suction, quick attach dump valve discharge hose. Truck is wired for 110 shore power with Kussmaul Electronics. Truck is piped for air inlet. Truck has a recent pump test in fall of 2023. Truck is 28' 10" long, 10' 8" High, wheel base is 18' 4" and GVWR is 56,000. Truck will be available in September of 2024 when new Tank Truck Arrives. We have had this truck appraised through Brindlee Mountain Fire Apparatus.

The asking price will be $50,000 obro. Truck can be viewed upon appointment.

Contact the Fire Chief via email: firechief@souththomaston.me or Cell: 207-542-4797.